Author: Valerie

Doug Kinsman
5328 Co Rd 22
Archbold, Ohio 43502
419-445-8605

High Tunnel– 30’ x 48’ Sandy Loam
Well PSI 50-60
GPH at hydrant: 480-600
Main supply line 20ft by 1/2”
Three Zones with in-line shut off valves for mixed specialty cropping in high tunnel.
Inline emitter tubing each approx. 42’ long– 1 gph on 12” spacing
Each zone (4 –42’ lines) 168 gallon gph capacity.

Hydrant

Brass Hose Y with swivel

Timer

Y Filter Hose Thread

Pressure regulator-30psi

Female hose beginning-Hose Thread to 1/2 “

Easy Loc Elbow

1/2” supply line tube

Easy Loc female tee

1/2” supply line
1/2” supply line

Shut off swivel valves

1/2” inline emitter tubing 12” spacing

Screw On End Caps

Doug Kinsman
5328 Co Rd 22
Archbold, Ohio 43502
419-445-8605

Hydrant

High Tunnel– 24’ x 24’ Sandy Loam
Well PSI 50-60
GPH at hydrant: 480-600
Main supply line 20ft by 1/2”
Three Zones with in-line shut off valves for mixed specialty cropping in high tunnel.
Inline emitter tubing each approx. 21’ long– 1 gph on 12” spacing
Each zone (3 –21’ lines)

Brass Hose Y with swivel

Timer

Filter/Pressure regulator-30psi

Easy Loc Elbow

1/2” supply line tube

Easy Loc female tee

1/2” supply line

Shut off swivel valves

1/2” inline emitter tubing 12” spacing

Screw On End Caps